IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2017-12-07T15:57:09"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20151007_0715(x64) - Exporter 16.4.0.0 - Alternate UI 16.4.0.0"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "connm" of Organization (no name given)
  Owner history of Person "connm" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT | long name "X:\NBL\Manufacturer\B\Betafence_7508\NBLA0794\Authoring\IFC\NBS_BetafenceLimited_MtlMeshPnlFncngSym_Nylofor3DProXL-Twilfix.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address: "St Nicholas Street, Newcastle Upon Tyne, UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nylofor 3D Pro XL + Twilfix" | object type "Nylofor 3D Pro XL + Twilfix" | names: "NBS_BetafenceLimited_MtlMeshPnlFncngSym_Nylofor3DProXL-Twilfix:Nylofor 3D Pro XL + Twilfix:137745" | material: materials ("NBS_BetafenceLimited_MtlMeshPnlFncngSym_Nylofor3DProXL_Panel", "NBS_Concept") | property sets: COBie

Types
  IFCBUILDINGELEMENTPROXYTYPE "Nylofor 3D Pro XL + Twilfix" | 1 occurrence | material: materials ("NBS_BetafenceLimited_MtlMeshPnlFncngSym_Nylofor3DProXL_Panel", "NBS_Concept") | property sets: NBS_General, NBS_Data, Pset_RailingCommon, IFC, COBie

Property sets
  COBie | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Ss_25_14_67_51: Metal mesh panel fencing systems" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Green (RAL 6005), black (RAL 9005)" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "n/a" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "PVC (in accordance with EN 10245 part 2 class 2b)" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "sales.sheffield@betafence.com" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Nylofor 3D Pro XL-Twilfix" (IFCTEXT)
    Name = "MetalMeshPanelFencingSystem_Nylofor3DProXL-Twilfix_BetafenceLimited" (IFCTEXT)
    NominalHeight = 2430. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_BetafenceLimited_MetalMeshPanelFencingSystem_Nylofor3DProXL-Twilfix" (IFCTEXT)
    ManufacturerName = "Betafence Limited" (IFCTEXT)
    ManufacturerURL = "www.betafence.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/3oqfmu2w" (IFCTEXT)
    NBSDescription = "Metal mesh panel fencing system" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "25-20-30/145" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "//www.betafence.co.uk/en/nylofor-3d-pro-xl" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Ss_25_14_67_51" (IFCTEXT)
    Uniclass2015Title = "Metal mesh panel fencing systems" (IFCTEXT)
    Uniclass2015Version = "Systems v1.6" (IFCTEXT)
    Version = "2" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Schools, infrastructure and transport, factories and logistics, public spaces and buildings" (IFCTEXT)
    BaseBoards = "n/a" (IFCTEXT)
    FenceTopping = "Cranked extension arm and connection piece or welded cranked arms" (IFCTEXT)
    PanelSizeOptions = "3000 x 1230 mm, 3000 x 1530 mm, 3000 x 1730 mm, 3000 x 1930 mm, 3000 x 2030 mm, 3000 x 2430 mm" (IFCTEXT)
    Panels = "Nylofor 3D Pro XL panels" (IFCTEXT)
    PostFoundations = "Installation guides available on request" (IFCTEXT)
    Posts = "Twilfix" (IFCTEXT)
    Rails = "n/a" (IFCTEXT)
    SiteAppliedFinishes = "Galvanised" (IFCTEXT)
    SystemAccessories = "Concrete plate holder, cranked extension arm and connection piece or welded cranked arms, security devices" (IFCTEXT)
  Pset_RailingCommon | properties | on 1 type object
    Diameter = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2430. (IFCLENGTHMEASURE) [MILLI METRE]
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcWallType" (IFCTEXT)
    IfcExportType = "NOTDEFINED" (IFCTEXT)