IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2019-03-04T11:58:06"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20171027_0315(x64) - Exporter 17.4.0.0 - Alternate UI 17.4.0.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "connm" of Organization (no name given)
  Owner history of Person "connm" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCWALL | type IFCWALLTYPE "NBS_BetafenceLimited_MtlMeshPnlFncngSym_PaladinClassic-Twilfix:Paladin Classic + Twilfix" | object type "NBS_BetafenceLimited_MtlMeshPnlFncngSym_PaladinClassic-Twilfix:Paladin Classic + Twilfix:19161" | names: "NBS_BetafenceLimited_MtlMeshPnlFncngSym_PaladinClassic-Twilfix:Paladin Classic + Twilfix:45652" | material: "NBS_BetafenceLimited_MtlMeshPnlFncngSym_PaladinClassic_Panel" | property sets: COBie

Types
  IFCWALLTYPE "NBS_BetafenceLimited_MtlMeshPnlFncngSym_PaladinClassic-Twilfix:Paladin Classic + Twilfix" | 1 occurrence | material: "NBS_BetafenceLimited_MtlMeshPnlFncngSym_PaladinClassic_Panel" | property sets: NBS_General, NBS_Data, Pset_RailingCommon, IFC, COBie

Property sets
  COBie | properties | on 1 object (1 IFCWALL)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Ss_25_14_67_51:Metal mesh panel fencing systems" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Green (RAL 6005), black (RAL 9005)" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Perimeter security" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "sales.sheffield@betafence.com" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Paladin Classic Twilfix" (IFCTEXT)
    Name = "MetalMeshPanelFencingSystem_PaladinClassicTwilfix_BetafenceLimited" (IFCTEXT)
    NominalHeight = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 3025. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_BetafenceLimited_MetalMeshPanelFencingSystem_PaladinClassic-Twilfix" (IFCTEXT)
    ManufacturerName = "Betafence Limited" (IFCTEXT)
    ManufacturerURL = "www.betafence.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/vnrst3ih" (IFCTEXT)
    NBSDescription = "Metal mesh panel fencing system" (IFCTEXT)
    NBSReference = "25-20-30/145" (IFCTEXT)
    ProductInformation = "www.betafence.co.uk/en/paladin-classic" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Ss_25_14_67_51" (IFCTEXT)
    Uniclass2015Title = "Metal mesh panel fencing systems" (IFCTEXT)
    Uniclass2015Version = "Systems v1.13" (IFCTEXT)
    Version = "3" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Company premises, public spaces, schools, retail, factories" (IFCTEXT)
    BaseBoards = "n/a" (IFCTEXT)
    FenceTopping = "n/a" (IFCTEXT)
    PanelSizeOptions = "3025 x 1240 mm, 3025 x 1850 mm, 3025 x 2000 mm, 3025 x 2440 mm" (IFCTEXT)
    Panels = "n/a" (IFCTEXT)
    PostFoundations = "Installation guides available on request" (IFCTEXT)
    Posts = "Twilfix" (IFCTEXT)
    Rails = "n/a" (IFCTEXT)
    SiteAppliedFinishes = "n/a" (IFCTEXT)
    SystemAccessories = "Concrete plate holder, cranked extension arm and connection piece or welded cranked arms, security devices" (IFCTEXT)
  Pset_RailingCommon | properties | on 1 type object
    Diameter = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcWallType" (IFCTEXT)
    IfcExportType = "NOTDEFINED" (IFCTEXT)