IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2017-12-12T11:01:00"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20151007_0715(x64) - Exporter 16.4.0.0 - Alternate UI 16.4.0.0"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "connm" of Organization (no name given)
  Owner history of Person "connm" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 1512664267 (2017-12-07T16:31:07Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT | long name "X:\NBL\Manufacturer\B\Betafence_7508\NBLA0794\Authoring\IFC\NBS_BetafenceLimited_SStlGts_Robusta_Single.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address: "St Nicholas Street, Newcastle Upon Tyne, UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCDOOR | type IFCDOORSTYLE "Robusta Single Leaf" | object type "Robusta Single Leaf" | names: "NBS_BetafenceLimited_SStlGts_Robusta_Single:Robusta Single Leaf:144983" | material: materials ("NBS_Concept", "NBS_BetafenceLimited_MtlMeshPnlFncngSym_Nylofor2D_Panel") | property sets: COBie

Types
  IFCDOORSTYLE "Robusta Single Leaf" | SINGLE_SWING_RIGHT | HIGH_GRADE_STEEL | 1 occurrence | material: materials ("NBS_Concept", "NBS_BetafenceLimited_MtlMeshPnlFncngSym_Nylofor2D_Panel") | property sets: NBS_BetafenceLimited_SStlGts_Robusta_Single:Robusta Single Leaf:144983, NBS_General, NBS_Data, Pset_RailingCommon, IFC, COBie

Property sets
  COBie | properties | on 1 object (1 IFCDOOR)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_30_59_34_80: Stainless steel gates" (IFCTEXT)
    CodePerformance = "CE Marking" (IFCTEXT)
    Color = "Green (RAL 6005), black (RAL 9005)" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Gate for perimeter security" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Polyester coating" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "sales.sheffield@betafence.com" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Robusta Single Leaf" (IFCTEXT)
    Name = "MetalMeshPanelFencingSystem_RobustaSingleLeaf_BetafenceLimited" (IFCTEXT)
    NominalHeight = 2072. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 985. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "To be taken from CAD" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "10 years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  NBS_BetafenceLimited_SStlGts_Robusta_Single:Robusta Single Leaf:144983 | predefined | on 2 type objects
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_BetafenceLimited_StainlessSteelGates_Robusta_Single" (IFCTEXT)
    ManufacturerName = "Betafence Limited" (IFCTEXT)
    ManufacturerURL = "www.betafence.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/ozwsw4ow" (IFCTEXT)
    NBSDescription = "Stainless steel gates" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-25-35/313" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "//www.betafence.com/en/robusta-medium" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_30_59_34_80" (IFCTEXT)
    Uniclass2015Title = "Stainless steel gates" (IFCTEXT)
    Uniclass2015Version = "Products v1.6" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    AccessControl = "n/a" (IFCTEXT)
    Applications = "Industry, situations where access control is recommended" (IFCTEXT)
    GateLeaves = "n/a" (IFCTEXT)
    HardwareHinges = "n/a" (IFCTEXT)
    HardwareOperating = "n/a" (IFCTEXT)
    HardwareSecuring = "n/a" (IFCTEXT)
    Posts = "steel: Type S235 JRH class 1, in accordance with EN 10219-2" (IFCTEXT)
    SecurityLevel = "Maximum Security" (IFCTEXT)
  Pset_RailingCommon | properties | on 1 type object
    Diameter = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2072. (IFCLENGTHMEASURE) [MILLI METRE]
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcDoorType" (IFCTEXT)
    IfcExportType = "GATE" (IFCTEXT)